It is good practice to regularly calibrate sprayers following manufacturers’ instructions. All PPP application equipment should be calibrated between seasons of use. Equipment used to apply granular PPPs and/ or slug pellets should be calibrated whenever there is a change of product.

Below is a template for recording calibration checks.

|  |  |  |  |
| --- | --- | --- | --- |
| **PPP application equipment** | **Date of calibration check** | **Details / Results / follow up actions** | **Operator name** |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |